Hamo® T-420 Glassware Washer
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Cleaning and Drying System

Wash chamber:

1290 x 700 x 800 mm (50¾ x 27½ x 31½ inches) and
             1290 x 1000 x 800 mm (50¾ x 39¼ x 31½ inches)
             (WxHxD)

The economical system for cleaning and drying of laboratory items.

Most Frequent Applications: 
The Hamo T-420 was developed specifically for the high demands of research laboratories. The machine is designed for cleaning the following parts: 

· Glassware 

· Drums and containers 

· Machine parts 

Details:
Extensive variants of equipment
- Single or double door machine
- Tank-independent rinsing 
- Monitoring of temperature and conductivity
- Rotation of the wash load
- Use of hollow jets with contact coupler to the basket
- High capacity HEPA filtered drying system 
- Ex-protection construction
- Barcode reader
- Wide variety of standard and custom designed baskets
- Extensive automation and conveyors

User-friendly control concept
- Microprocess control Infracontrol with Editor on external PC
- RS 232 Interface for SCADA

Real-time process-documentation
- System for documentation of process data visualization (PDVS) 
- Data availability on printer, network, and data mediums 

